  Please Mail Comments	 Owner	           						 Date Received: _________ By: _________
  Will Pick Up Comments	 Applicant
	  				 GENERAL APPLICATION
MURRAYHILL ARCHITECTURAL REVIEW COMMITTEE (ARC) 
________________________________________________________________________________________________________________________________

Lot Number: ______ Lot Address: __________________________________________________________________________
Owner _______________________________________________________ Owners Phone: ____________________________
Owner Address: ________________________________________________Work Phone: ______________________________
E-mail; Address: _______________________________________________ Cell Phone: _______________________________
Contractor/Designer: ____________________________________________ Contactors Phone:  _________________________

Application For:	
    Construction Prelim. Review - $35.00	  Fence/Screening - $35.00			Gazebo, Shed, etc. - $60.00
    New Construction Review - $1,500	  Deck/Patio/Flatwork. - $60.00	 	Retaining Walls - $60.00		
    Doors & Windows - $35.00		  Play Structure – $35.00	        		Landscape Renovation - $60.00    

    Remodel – Minimum $300.00 or                  Spa - $60.00				Tree Removal - $60.00	  

     $1.00 per square foot  		                 Recreation Equip. - $60.00		Other_______________
    		  					 
 	      
Exterior:  Paint, Brick, Re-siding, Exterior/Landscape Lighting, and Solar Roof Devices require a separate form. 
	    
 $                         Total Application fees
 Please see additional information on the back of this form. 
As an applicant for Design Review, I/we have read the current Murrayhill Covenants, Conditions, & Restrictions (CC&R’s) and Design Guidelines and the application and fully understand the requirements of this construction application.  Any change in the exterior from an approved application must be resubmitted to the Architectural Review Committee for approval prior to beginning work.
I assume responsibility for any and all damage caused by my construction to adjacent lots, common areas, or my/our property.
	
Submittal of this application is the authority for the ARC or agent to make on-site observations, including taking photographs, etc., of the lot and/or home as part of the review process and to determine reasonable compliance with approved applications.

Owner Signature:_____________________________________________Date:______________________

	


Committee Action

Date:     ____________	      	  Approved Review as proposed		____________________________________
Expires:  ___________		  Approved with Conditions		____________________________________
				  Sent Back (Please see comments)		____________________________________
This is your approval if signed by three members of the ARC.

	


REVIEW COMMENTS AND/OR APPROVAL CONDITIONS

																																																											
PROCEDURES FOR OBTAINING ARC APPROVAL

Please submit plans and completed application form to the ARC Administrator at the Murrayhill Owners Association office.  INCOMPLETE 
APPLICATIONS WILL BE RETURNED WITHOUT REVIEW.   Applicants will be notified as soon as review is complete.
If you have a question about the Architectural Review Committee process, please call the MOA office at 503-524-4429 or email us at admin@murrayhillowners.com.

Return all applications to the MOA office at 11010 SW Teal Blvd., Beaverton, OR 97007

DRAWING REQUIREMENTS


SITE PLAN	
-  scale 1/8”=1’
-  existing grade, 2’ interval
-  building outline
-  finish grades, 2’ interval
-  north arrow
-  trees to be cut
-  trees to remain
-  street names
-  utility meters
-  patios, decks, walks
-  service yards
-  fences, screens, details
-  drainage patterns
-  retaining walls
-  setbacks, easements
-  property lines, 
   dimensions
-  driveways,
-  stairs

FLOOR PLANS
-  scale 1/8”=1’ (minimum)
-  doors, windows (size,   
    operating type)                     
-  room names
-  stairways
-  exterior lighting locations
-  square feet by floor
-  location of trash storage 
    area


BUILDING ELEVATIONS
-  scale 1/8”=1’ (minimum)
-  roof and material
-  siding material
-  siding direction
-  chimney chases
-  window operation
-  muntin bar pattern
-  finish floor lines
-  trim, corner boards
-  railings, decks, stairs
-  below deck screening
-  vents and flues
-  location, pattern of brick
-  garage door size
-  accurate finish grades


LANDSCAPE PLANS
-  scale 1/8”=1’ (minimum)
-  planter areas, mulch
-  plant common name
-  plant botanical name
-  plant size at planting
-  mature size drawn to 
   scale
-  north arrow
-  berms, grading
-  retaining walls
NOTE:  Approved plans are returned to owner, if owner is applicant.  If applicant is other than owner, and owner wishes a copy of approved plans, please provide 3 copies of all materials sent in for review (plans, specifications, etc.).


EXTERIOR LIGHTING
Please submit 1 copy of the approved form including catalog cuts or legible copies from catalogs indicating all exterior light fixtures.  Indicate overall height, material finishes and locations.  See form titled “EXTERIOR LIGHTING” for additional information.

EXTERIOR COLORS
Please submit 2 copies of the approved form including samples of all exterior colors for each exterior material.  Larger samples of actual color (mock-ups) on actual material or house may be required by the ARC prior to final approval.  See form titled “EXTERIOR COLORS” for additional information.

EXTERIOR BRICK
Unless a brick sample is already on file with the ARC, please submit an actual sample of the proposed brick indicating the typical blend expected.  See form titled “SIDING, BRICK, STONE” for additional information.

ITEMS TO REMEMBER
Both Preliminary Approval and Final Construction Approval are valid for 180 days.  If construction has not begun in that time, a new application must be made, and will require a second fee.

All proposed construction on the lot must be completed within 270 days from the date construction is begun, unless otherwise approved by the ARC.  Front yard landscaping must be completed within 90 days of completion of construction; back yard within 180 days.

Gas vents, flues:  behind ridges, painted to match weathered roof color or tile/comp. roofing color.

Decks:  underside screened if more than 24” to grade with lattice or landscaping.  See standard detail.

Brick:  standard size at wall veneer, econs at chimneys if separate from veneer by at least 3’.

Siding:  overlaid waferwood or cedar, joints caulked or with matching joint covers.  Stucco-like plywood panels may be acceptable if no panel edges are exposed and pattern of battens is regular and logical.

Garage doors:  raised panel wood or embossed panel metal.

Please see Murrayhill CC&Rs as stated in section 5.3, Design Review Procedure for completion notice.


